{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":6,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["工程预算分类","类别","定额名称","单位","综合单价","项目说明"]
["土木","2022班平层泥水工程","墙面批荡按单面计算","平方",116,"华润-润丰”PC牌32.5水泥、沙(水泥沙浆标准厚度为40mm，厚度每增加10mm，单价增加5元/㎡)、工字形/斜铺加20元每平方。含人工、辅料。地砖、定位卡业主提供。填缝费用另计。"]
["土木","2022班平层泥水工程","安装门槛石《单扇不超1M)","米",300,"德高瓷砖胶，含人工、辅料；地砖、定位卡业主提供，填缝费用另计。工字形/斜铺加20元每平方。（此规格以上地砖均采用薄贴工艺，原地面须冲筋找平，费用另计）"]